# Stakeholders

| Stakeholder name | Description |

| RVC User | :Final user of the system: |

| RVC Company | :Includes software/electrical/mechanical engineers, marketing people…:|

| RVC Retailer | :Store that buys from company and sells to final users: |


| RVC Maintainer | :Technicians for installation and maintenance: |

| Certification Authority | :Entity that issues safety/energy certificates: |

| Obstacles | :Walls, objects, animals, doors… |

# Context diagram and interfaces

## Context diagram



## Interfaces

| Actor | Physical interface | Logical interface |

| End user | :On/Off switch: Start switch: Learn switch: | :On/Off command: Start command: Learn command: |

| Power socket | :Shuko standard: | :220V 50 Hz:|

| Obstacle | IR sensor | Detect obstacle |

# Functional and Non-Functional requirements

## Functional requirements